RT_USING_MTD_NOR (defined at D:\new1\SiFli-SDK//rtos/rtthread/components/drivers/Kconfig:122) was assigned the value 'y' but got the value 'n'. Check these unsatisfied dependencies: BSP_USING_RTTHREAD (=n). 
