# SF32LB58-LCD_A128R32N1_DSI
`sf32lb58-lcd_a128r32n1_dsi` board is based on SF32LB58-DevKit-LCD board and 
has module [SF32LB58-MOD-A128R32N1](https://wiki.sifli.com/silicon/%E6%A8%A1%E7%BB%84%E5%9E%8B%E5%8F%B7%E6%8C%87%E5%8D%97.html#sf32lb58-mod) on the board. 
`8.0 rect DSI Video TFT LCD(800x1280 TFT-H080A11HDIFT4C30_V0-1)` with DSI interface is used as default display.

![board front side](assets/SF32LB56x-DevKit-LCD_Front_Look.png)